Printed concrete, thickness= 10cm

Crushed stone material 0-31.5, thickness=10 cm

Gravel, thickness=20cm

Road verge made od gravel

Level

Distance

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Designer:    Engineering activities and  technical consultancy,  Dragan Peric,  Bulevar Nemanjica no. 27/11, 18000 Nis | Investor: | City Municipality Crveni Krst- City of Nis | | | |
| Mark of technical documents: | IDP | Project:  CONCEPTUAL DESIGN | MARKS OF WORK PROJECT: 2/2 | |
| Chief Designer:  dr Dragan Peric,  Civil engeener,  License number:  315 0982 03 | Stamp: | Object:  Pedestrian pathway in village Miljkovac, City municipality Crveni Krst | | |
| Date:  . | | Drawing name: | | Scale:  1:100/1000 |
| 30. November 2015 | | Specific cross-section | | Number of drawing:  41 |