PR37

F excavation= 0.28

F mound = 0.00

F verge road= 0.17

L pos = 3.09

L subsoil = 0.00

F buffer 1 = 0.16

F buffer 2 = 0.83

F excavation of humus= 0.64

L concrete = 1.20

Level

Distance

PR38

F excavation= 0.20

F mound = 0.00

F verge road= 0.17

L pos = 2.46

L subsoil = 0.00

F buffer 1 = 0.16

F buffer 2 = 0.26

F excavation of humus= 0.49

L concrete = 1.20

Level

Distance

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Designer:    Engineering activities and  technical consultancy,  Dragan Peric,  Bulevar Nemanjica no. 27/11, 18000 Nis | Investor: | City Municipality Crveni Krst- City of Nis | | | |
| Mark of technical documents: | IDP | Project:  CONCEPTUAL DESIGN | MARKS OF WORK PROJECT: 2/2 | |
| Chief Designer:  dr Dragan Peric,  Civil engeener,  License number:  315 0982 03 | Stamp: | Object:  Pedestrian pathway in village Miljkovac, City municipality Crveni Krst | | |
| Date:  . | | Drawing name: | | Scale:  1:100/1000 |
| 30. November 2015 | | Cross section | | Number of drawing:  11 |