Detail of making concrete border BNHS- 16 , thickness=6 cm with roadside 12/18 on the concrete layer

Concrete border with roadside 12/18 cm

BNHS- 16 , thickness=7 cm

CRUSHED STONE MATERIAL 0-31, thickness=10 cm

Gravel, thickness=15 cm

Existing fence

Gravel verge

LEVEL

DISTANCE

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Designer:    Engineering activities and  technical consultancy,  Dragan Peric,  Bulevar Nemanjica no. 27/11, 18000 Nis | Investor: | City Municipality Crveni Krst- City of Nis | | | |
| Mark of technical documents: | IDP | Project:  CONCEPTUAL DESIGN | MARKS OF WORK PROJECT: 2/2 | |
| Chief Designer:  dr Dragan Peric,  Civil engeener,  License number:  315 0982 03 | Stamp: | Object:  Pedestrian pathway in village Miljkovac, City municipality Crveni Krst | | |
| Date: | | Drawing name: | | Scale:  1:50 |
| 03. December, 2015 | | Specific  cross-section | | Number of drawing:  41/1 |