PR1

F excavation= 4.03

F mound = 0.00

F verge road= 0.15

L pos = 7.00

L subsoil = 0.00

F buffer 1 = 0.64

F buffer 2 = 1.38

F canal= 0.00

L BNS = 6.00

Level

Distance

PR2

F excavation=0.40

F mound = 0.00

F verge road= 0.15

L pos = 2.20

L subsoil = 0.00

F buffer 1 = 0.16

F buffer 2 = 0.00

F canal= 0.00

L concrete = 1.20

Level

Distance

PR3

F excavation= 0.93

F mound = 0.00

F verge road= 0.15

L pos = 2.20

L subsoil = 0.00

F buffer 1 = 0.16

F buffer 2 = 0.00

F canal= 0.00

L concrete = 1.20

Level

Distance

PR4

F excavation=0.20

F mound = 0.39

F verge road= 0.15

L pos = 2.40

L subsoil = 2.05

F buffer 1 = 0.16

F buffer 2 = 0.00

F canal= 0.00

L concrete = 1.20

Level

Distance

PR5

F excavation=0.60

F mound = 1.10

F verge road= 0.25

L pos = 3.04

L subsoil = 2.33

F buffer 1 = 0.16

F buffer 2 = 0.00

F canal= 0.00

L concrete = 1.20

Level

Distance

PR6

F excavation=0.43

F mound = 0.00

F verge road= 0.18

L pos = 2.20

L subsoil = 0.00

F buffer 1 = 0.16

F buffer 2 = 0.00

F canal= 0.00

L concrete = 1.20

Level

Distance

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Designer:    Engineering activities and  technical consultancy,  Dragan Peric,  Bulevar Nemanjica no. 27/11, 18000 Nis | Investor: | City Municipality Crveni Krst- City of Nis | | | |
| Mark of technical documents: | IDP | Project:  CONCEPTUAL DESIGN | MARKS OF WORK PROJECT: 2/2 | |
| Chief Designer:  dr Dragan Peric,  Civil engeener,  License number:  315 0982 03 | Stamp: | Object:  Pedestrian pathway in village Miljkovac, City municipality Crveni Krst | | |
| Date: | | Drawing name: | | Scale:  1:100/1000 |
| 03. December, 2015 | | Cross section | | Number of drawing:  38 |